{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["FAQ and Tips"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FAQ and Tips","index":0,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Question or Area of Concern"," Description"," Solution"," Author"]
["Potable Water Fill"," How can I get the water to automatically shut off when tank is full"," Use a garden flowmeter which measures the gallons which go thru it and shut off."," Rich D.  99 Lxi 43"]
["Can't find Water Pump"," Looking all over 80 FC and can't find the pump"," Pump is located in Bath inside the lower cabinet under floor next to toilet"," Les Grey 80FC"]
["Glue for Vinyl on Ceilings"," Re-glueing vinyl to ceiling panels doesn't hold"," Use 3M 8090 Glue (for heavy materials) and make sure glue is applied to both surfaces and dries tack free before bonding"," Lee Condosta, Wilmington, NC (3M Jobber)"]
["Fuel Tank Capacity Formula"," How to calculate fuel capacity from tank measurements"," Measure tank in inches: W x L x H...divide by 231 = Gallons.  Reduce each measurement by 1/4 inch to compensate for the wall thickness"," Curt Sprenger"]
["Horton Engine Cooling Fan"," Fan cuts on & off frequently or stays on when temp is low.  Air release sound heard"," Check for loose wire to or bad  KYSOR Temp Sensor on block"," Jeff Miller"]
["SP 36 Runs Warm"," Oil and dirt have accumulated on radiator and aftercooler from crankcase breather"," Wash radiator thoroughly after soaking with mild soap (Dawn,Simple Green,Oil Eater),extend oil breather tube out beyond radiator with 1 inch tube or hose"," Fred Hulse"]
["Engine idling of 2 stroke DD"," DD 2 strokes don't move enough air to keep carbon specks from being deposited in the air cleaner & intoduced into the cylinders when rpms raised to drive."," Don't idle for more than 3 minutes with DD - same is not true for 4 stroke engines"," George Lowry, WA"]
["Satellite fails for in-motion units"," Satellite cannot lock onto target when wired into coach 12v system"," Purchase a 13.8v power supply with good filtering to power system"," John Sutter"]
["FC Suspension ride height adjustment"," How do you adjust the ride height on an FC"," If you measure from the skirt to the ground behind the front axle should be 19 inches and in front of the rear axle should be 20 inches."," Bruce Morris"]
["Pure Water Tank"," Add a cleanout port to the water tank for access and adding chlorine"," Jack M. ... VB128 ...As a result of disuse, water from my fresh water storage tank developed an objectionable odor and taste even though I drained the tank each time the coach was not being used. I tried Algae - Kill, Clorox, swimming pool chlorine and everything else I could find with little or no success. I could not get the tanks clean and sweet. I cut a hole in the top of the fresh water tank, to accept removable deck plates. When I opened the tank I found the inside coated with a brown algae predominately on the top and corner surfaces. I scrubbed the entire tank clean with a scrub brush and thoroughly rinsed it. In the future I will be able to inspect and clean it as needed through the deck plates. I used the following parts: Beckson Deck Plates # DP60-W 6, Inspection plates $14.00 and #BKS - DP60W - Deck plate $11.50 These parts were purchased from Beckson Marine Inc. Box 3336, Bridgeport, CT 06605"," Jack M."]
["Sealing Roof Leaks"," Some places on roof are difficult to seal because of obstructions, etc."," Use Dicor sealant available in caulking tubes at most RV stores.  It is rubberized, flowing and self-leveling"," David Hollis  78 FC33"]
["Flourescent Lights"," How can you remove the bulbs easily?"," Use a flat jar gripper by putting it over the bulb and pinching the bottom edges together and turn the bulb"," Sid Clark 85PT36"]
["Engine Coolant Leak"," Coolant leaks from small hose going to beer can canister under passenger side of frame"," Check annually and replace as needed"," Lee Benson 85FC35"]
["Fuel Blowback  solution"," Diesel fuel always blows back out before hose shuts off"," Get 6 ft. of 1.5 thinwall schedule 20 pcv pipe and put it in the tank as far as it will go.  Cut it off about 1 below filler neck.  Works Great!"," Elmer 86 PT 38 in Florida"]